Product details:

Model number: SMT-1200

Chapati Capacity: 1200 nos/ Hr

LPG consumption: 2-2.5 kg/Hr

Electricity: 1.5 KW/Hr

Machine weight : 255 kg

Weight of chapati : 25 to 55 Gms

Size of chapati : 4” to 9”

Overall dimension: 5.8’ (L) \* 4’ (W) \* 3.5’ (H)

Thickness of chapati : 1 to 2.5mm

Gas pressure: Normal

The automatic chapati making machine boasts of being the india"s best easy automatic chapati making machine with a capacity to cook 1200 chapatis in one hour. , the machine is used by leading caterers, hotel, school, aashram and restaurants to cook chapati, even at outdoor catering locations. With great mobility, compact size and low gas and electricity requirements, the machine serves as an ideal chapati making solution for the F&B industry.